(module Fuse_SMD1206 (layer F.Cu) (tedit 56DED6ED)
  (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
  (tags "Fuse, Sicherung, SMD1206,  Littlefuse-Wickmann 433 Series, Hand Soldering,")
  (attr smd)
  (fp_text reference REF** (at -0.0508 -2.19964) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Fuse_SMD1206 (at -0.14986 2.49936) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.81 -1.27) (end -3.81 -1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.81 1.27) (end 3.81 -1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.81 1.27) (end 3.81 1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.81 -1.27) (end -3.81 1.27) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -2.08534 0 90) (size 2.02946 2.65176) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.08534 0 90) (size 2.02946 2.65176) (layers F.Cu F.Paste F.Mask))
)
