(module DIPS4 (layer F.Cu) (tedit 57151A76)
  (fp_text reference REF** (at 7.0358 0.1016 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value >NAME (at -7.4676 -0.0762 90) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5 2) (end 5 -2) (layer Cmts.User) (width 0.15))
  (fp_line (start -5 2) (end 5 2) (layer Cmts.User) (width 0.15))
  (fp_line (start -5 -2) (end -5 2) (layer Cmts.User) (width 0.15))
  (fp_line (start 5 -2) (end -5 -2) (layer Cmts.User) (width 0.15))
  (fp_line (start -6 2) (end -5 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 2) (end -6 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 3) (end -5 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 -3) (end 6 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -3) (end 6 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 -4) (end -7 -4) (layer Eco1.User) (width 0.15))
  (fp_line (start 7 4) (end -7 4) (layer Eco1.User) (width 0.15))
  (fp_line (start 7 4) (end 7 -4) (layer Eco1.User) (width 0.15))
  (fp_line (start -7 4) (end -7 -4) (layer Eco1.User) (width 0.15))
  (pad 7 smd rect (at -1.27 -4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.27 -4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.27 4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1.27 4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -3.81 -4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 3.81 -4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 3.81 4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.81 4.3) (size 1.12 2.44) (layers F.Cu F.Paste F.Mask))
)
