(module USB3_AFEMALE_MOD (layer F.Cu) (tedit 57151E03)
  (descr USB1070)
  (tags USB1070)
  (attr smd)
  (fp_text reference REF** (at 0 -12.446) (layer F.SilkS)
    (effects (font (thickness 0.3048)))
  )
  (fp_text value >NAME (at 0.0508 5.2324) (layer F.SilkS) hide
    (effects (font (thickness 0.3048)))
  )
  (fp_text user "Mating Distance" (at -2.032 7.112) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6.731 -11) (end 6.731 -11) (layer Cmts.User) (width 0.15))
  (fp_line (start -7.25 3.5) (end 7.25 3.5) (layer Cmts.User) (width 0.15))
  (fp_line (start 7.25 3.25) (end 7.25 3.5) (layer Cmts.User) (width 0.15))
  (fp_line (start 6.731 3.25) (end 7.25 3.25) (layer Cmts.User) (width 0.15))
  (fp_line (start 6.731 -11) (end 6.731 3.25) (layer Cmts.User) (width 0.15))
  (fp_line (start -6.731 3.25) (end -7.25 3.25) (layer Cmts.User) (width 0.15))
  (fp_line (start -7.25 3.5) (end -7.25 3.25) (layer Cmts.User) (width 0.15))
  (fp_line (start -6.731 -11) (end -6.731 3.25) (layer Cmts.User) (width 0.15))
  (fp_line (start 6.731 -8.509) (end -6.731 -8.509) (layer Dwgs.User) (width 0.1016))
  (fp_line (start -6.731 -8.509) (end -6.731 0) (layer Dwgs.User) (width 0.1016))
  (fp_line (start 6.731 0) (end 6.731 -8.509) (layer Dwgs.User) (width 0.1016))
  (fp_line (start -8 6.2) (end 8 6.2) (layer Cmts.User) (width 0.15))
  (fp_line (start -9 -12) (end 9 -12) (layer Eco1.User) (width 0.15))
  (fp_line (start -9 4) (end 9 4) (layer Eco1.User) (width 0.15))
  (fp_line (start -9 -12) (end -9 4) (layer Eco1.User) (width 0.15))
  (fp_line (start 9 -12) (end 9 4) (layer Eco1.User) (width 0.15))
  (pad 10 thru_hole oval (at 7.9 -9) (size 1.8 3.5) (drill oval 0.6 2.2) (layers *.Cu *.Mask F.Paste F.SilkS))
  (pad 10 thru_hole oval (at -7.9 -9) (size 1.8 3.5) (drill oval 0.6 2.2) (layers *.Cu *.Mask F.Paste F.SilkS))
  (pad 7 smd rect (at 0 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 3 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 4 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -2 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -4 -9.9) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 7.67 -5) (size 1.64 2.2) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -7.67 -5) (size 1.64 2.2) (layers F.Cu F.Paste F.Mask))
  (model 3d/usb3afemale_mid.wrl
    (at (xyz 0 0.195 0))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz 90 180 0))
  )
)
