(module 00Keyboard:HC-49_SMT (layer F.Cu)
  (fp_text reference HC-49_SMT (at 0 -3.4) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value VAL** (at 0 3.4) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start -6 -2.4) (end 6 -2.4) (layer F.SilkS) (width 0.2))
  (fp_line (start 6 -2.4) (end 6 2.4) (layer F.SilkS) (width 0.2))
  (fp_line (start 6 2.4) (end -6 2.4) (layer F.SilkS) (width 0.2))
  (fp_line (start -6 2.4) (end -6 -2.4) (layer F.SilkS) (width 0.2))
  (pad 1 smd rect (at -4.75 0) (size 5.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 4.75 0) (size 5.5 2) (layers F.Cu F.Paste F.Mask))
)
