(module JST_PH2_SMT_TH (layer F.Cu)
  (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
  (tags "JST, PH, Lipo, battery")
  (fp_text reference JST_PH2_SMT (at 1.2 2.9) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value VAL** (at 1.4 -3.6) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start -2.9 -0.4) (end -2.9 4) (layer F.SilkS) (width 0.2))
  (fp_line (start -2.9 -0.4) (end 4.9 -0.4) (layer F.SilkS) (width 0.2))
  (fp_line (start 4.9 -0.4) (end 4.9 4) (layer F.SilkS) (width 0.2))
  (fp_line (start 3.6 7.2) (end -1.6 7.2) (layer F.SilkS) (width 0.2))
  (pad 3 smd rect (at 5.1 5.95) (size 1.5 3.4) (drill (offset -0.75 -0.2)) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2 0) (size 1 3.5) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.6 5.95) (size 1.5 3.4) (drill (offset -0.75 -0.2)) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0 0) (size 1 3.5) (layers F.Cu F.Paste F.Mask))
  (pad 2 thru_hole oval (at 2 2) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole oval (at 0 2) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
)
