(module SOLDER_JUMPER_3 (layer F.Cu) (tedit 54860828)
  (tags "solder jumper bridge configuration")
  (attr virtual)
  (fp_text reference JP*** (at 0 -1.7) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value SOLDER_JUMPER_3 (at 0 1.65) (layer F.SilkS) hide
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start 1.35 -0.55) (end 1.35 0.6) (layer F.SilkS) (width 0.2))
  (fp_line (start -1.1 -0.85) (end 1.1 -0.85) (layer F.SilkS) (width 0.2))
  (fp_line (start -1.35 0.6) (end -1.35 -0.6) (layer F.SilkS) (width 0.2))
  (fp_line (start -1.05 0.85) (end 1.1 0.85) (layer F.SilkS) (width 0.2))
  (fp_arc (start -1.1 0.6) (end -1.1 0.85) (angle 90) (layer F.SilkS) (width 0.2))
  (fp_arc (start -1.1 -0.6) (end -1.35 -0.6) (angle 90) (layer F.SilkS) (width 0.2))
  (fp_arc (start 1.1 -0.6) (end 1.1 -0.85) (angle 90) (layer F.SilkS) (width 0.2))
  (fp_arc (start 1.1 0.6) (end 1.35 0.6) (angle 90) (layer F.SilkS) (width 0.2))
  (pad 2 smd rect (at 0 0) (size 0.6 1.2) (layers F.Cu F.Mask)
    (clearance 0.1))
  (pad 3 smd rect (at 0.8 0) (size 0.6 1.2) (layers F.Cu F.Mask)
    (clearance 0.1))
  (pad 1 smd rect (at -0.8 0) (size 0.6 1.2) (layers F.Cu F.Mask)
    (clearance 0.1))
)
