(module Inductor_Bourn_4mmx4mm (layer F.Cu) (tedit 56EAD789)
  (fp_text reference REF** (at 0.1778 2.5654) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value >NAME (at 0 -2.794) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.4 2) (end -2.4 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.4 2) (end -2.4 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.4 -2) (end 2.4 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.4 -2) (end 2.4 -2) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -1.525 0) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.525 0) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask))
)
