(module USB_miniB_hirose_5ST_hand (layer F.Cu) (tedit 5485C0BC)
  (descr "USB miniB hirose UX60SC_MB_5ST")
  (tags "USB miniB hirose new")
  (fp_text reference J1 (at 0 2.45) (layer F.SilkS)
    (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
  )
  (fp_text value USB_miniB (at 0 7.95) (layer F.SilkS) hide
    (effects (font (thickness 0.3048)))
  )
  (fp_line (start -1 6.1) (end 1 6.1) (layer Dwgs.User) (width 0.2))
  (fp_line (start -3.85 6.6) (end -3.85 5.7) (layer Dwgs.User) (width 0.2))
  (fp_line (start 3.85 6.6) (end 3.85 5.7) (layer Dwgs.User) (width 0.2))
  (fp_text user "PCB edge" (at -0.05 5.35) (layer F.SilkS) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start -3.85 6.6) (end 3.85 6.6) (layer Dwgs.User) (width 0.2))
  (pad 1 smd rect (at -1.6 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.8 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.8 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.6 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -4.2 2.4) (size 2.5 4.2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 4.2 2.4) (size 2.5 4.2) (layers F.Cu F.Paste F.Mask))
)
