(module LED_TH_BIVAR (layer F.Cu) (tedit 593405F3)
  (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
  (tags "LED led 3mm 3MM 100mil 2,54mm")
  (fp_text reference LED*** (at 0 -1.9) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value LED_TH_BIVAR (at 0 2.032) (layer F.SilkS) hide
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user + (at 3.048 0) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (pad 1 thru_hole rect (at -1.27 0) (size 1.9 1.9) (drill 1.1176) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 1.27 0) (size 1.9 1.9) (drill 1.1176) (layers *.Cu *.Mask F.SilkS))
  (model ../../../../../home/dbroqua/Projects/dbroqua/DK60TP/Footprint/3D/LED-3MM.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
