(module USB3_MICROB (layer F.Cu) (tedit 57151D1D)
  (descr USB3110)
  (tags USB3110)
  (attr smd)
  (fp_text reference REF** (at 0.3302 -4.5974) (layer F.SilkS)
    (effects (font (thickness 0.3048)))
  )
  (fp_text value >NAME (at -0.889 4.3434) (layer F.SilkS) hide
    (effects (font (thickness 0.3048)))
  )
  (fp_line (start 6.325 -4) (end 6.325 3) (layer Eco1.User) (width 0.15))
  (fp_text user "Mating Distance" (at -2.667 4.826) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -7.175 1.45) (end 5.825 1.45) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7.175 2.75) (end -7.175 -3) (layer Cmts.User) (width 0.15))
  (fp_line (start 5.825 -3) (end 5.825 2.75) (layer Cmts.User) (width 0.15))
  (fp_line (start 5.825 -3) (end -7.175 -3) (layer Cmts.User) (width 0.15))
  (fp_line (start -7.175 2.75) (end 5.825 2.75) (layer Cmts.User) (width 0.15))
  (fp_line (start -8.675 4.05) (end 7.325 4.05) (layer Cmts.User) (width 0.15))
  (fp_line (start -7.675 3) (end 6.325 3) (layer Eco1.User) (width 0.15))
  (fp_line (start -7.675 -4) (end 6.325 -4) (layer Eco1.User) (width 0.15))
  (fp_line (start -7.675 -4) (end -7.675 3) (layer Eco1.User) (width 0.15))
  (pad 11 smd rect (at 0.65 0) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 3.35 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 4 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 4.65 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.7 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.05 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -3.35 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.7 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.05 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -4 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -4.65 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -4.55 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -2.15 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 11 thru_hole oval (at -6.95 0) (size 1.05 1.9) (drill oval 0.45 1.3) (layers *.Cu *.Mask F.Paste F.SilkS))
  (pad 11 smd rect (at 3.15 0) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 11 thru_hole oval (at 5.6 0) (size 1.05 1.9) (drill oval 0.45 1.2) (layers *.Cu *.Mask F.Paste F.SilkS))
  (model 3d/usb3microstakes.wrl
    (at (xyz -0.02 0.08 -0.038))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz -90 0 0))
  )
)
