(module WS2812B (layer F.Cu) (tedit 56CC5151)
  (descr "<b>Intelligent control LED with integrated light source</b><p>WS2812B<br>source: http://www.world-semi.com/uploads/soft/130904/1_1500205981.pdf")
  (solder_mask_margin 0.1)
  (attr smd)
  (fp_text reference WS2812B (at 6.35 0.0254) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value >NAME (at 5.778 1.2952) (layer Dwgs.User)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer Dwgs.User) (width 0.127))
  (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer Dwgs.User) (width 0.127))
  (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer Dwgs.User) (width 0.127))
  (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer Dwgs.User) (width 0.127))
  (fp_line (start -2.4892 -2.3622) (end -2.4892 -2.6162) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.4892 -2.6162) (end -2.4384 -2.6162) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.4384 -2.6162) (end -2.4384 -2.61112) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.4384 -2.61112) (end 2.51206 -2.61112) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.51206 -2.61112) (end 2.51206 -2.37998) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.50952 2.31902) (end -2.50952 2.5908) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.50952 2.5908) (end -2.45872 2.5908) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.45872 2.5908) (end -2.45872 2.59334) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.45872 2.59334) (end 2.50952 2.59334) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.50952 2.59334) (end 2.50952 2.36728) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.54 0.889) (end -2.54 -0.8128) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.54 -0.8636) (end 2.54 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.54 0) (end 2.54 0.8636) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.54 0) (end 0 2.54) (layer F.SilkS) (width 0.2032))
  (pad 1 smd rect (at -2.577 -1.6) (size 1.651 1) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.2))
  (pad 4 smd rect (at 2.577 -1.6) (size 1.651 1) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.2))
  (pad 3 smd rect (at 2.577 1.6) (size 1.651 1) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.2))
  (pad 2 smd rect (at -2.577 1.6) (size 1.651 1) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.2))
)
