(module USB_miniB_hirose_5S8 (layer F.Cu) (tedit 57C0F6FB)
  (descr "USB miniB hirose UX60SC-MB-5S8")
  (tags "USB miniB hirose through hole UX60SC-MB-5S8")
  (fp_text reference J1 (at 0 2.45) (layer F.SilkS) hide
    (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
  )
  (fp_text value USB_mini_micro_B (at 0 7.95) (layer Dwgs.User) hide
    (effects (font (thickness 0.3048)))
  )
  (fp_line (start 3.85 -0.4) (end 3.85 6.1) (layer F.SilkS) (width 0.2))
  (fp_line (start -3.85 -0.4) (end -3.85 6.1) (layer F.SilkS) (width 0.2))
  (fp_line (start -3.85 -0.4) (end 3.85 -0.4) (layer F.SilkS) (width 0.2))
  (fp_line (start -1 6.1) (end 1 6.1) (layer Dwgs.User) (width 0.2))
  (fp_line (start -3.85 6.6) (end -3.85 5.7) (layer Dwgs.User) (width 0.2))
  (fp_line (start 3.85 6.6) (end 3.85 5.7) (layer Dwgs.User) (width 0.2))
  (fp_text user "PCB edge" (at -0.05 5.35) (layer Dwgs.User) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start -3.85 6.6) (end 3.85 6.6) (layer Dwgs.User) (width 0.2))
  (pad 1 smd rect (at -1.6 0) (size 0.5 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.8 0) (size 0.5 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 0) (size 0.5 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.8 0) (size 0.5 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.6 0) (size 0.5 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 thru_hole oval (at -3.65 2.4) (size 1.3 3.8) (drill oval 0.7 3.2) (layers *.Cu *.Mask F.Paste))
  (pad 6 thru_hole oval (at 3.65 2.4) (size 1.3 3.8) (drill oval 0.7 3.2) (layers *.Cu *.Mask F.Paste))
)
