(module BreakHoles (layer F.Cu) (tedit 59DA336C)
  (fp_text reference BREAKHOLES1 (at 0 1.4732) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MISC (at 0 -1.4224) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "" np_thru_hole circle (at 0 142.24) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 140.97) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 138.43) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 137.16) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 135.89) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 134.62) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 132.08) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 130.81) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 129.54) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 128.27) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 125.73) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 124.46) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 123.19) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 121.92) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 119.38) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 118.11) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 116.84) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 115.57) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 113.03) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 111.76) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 110.49) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 109.22) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 106.68) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 105.41) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 104.14) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 102.87) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 100.33) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 99.06) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 97.79) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 96.52) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 93.98) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 92.71) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 91.44) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 90.17) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 87.63) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 86.36) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 85.09) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 83.82) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 81.28) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 80.01) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 78.74) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 77.47) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 74.93) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 73.66) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 72.39) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 71.12) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 68.58) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 67.31) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 66.04) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 64.77) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 62.23) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 60.96) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 59.69) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 58.42) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 55.88) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 54.61) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 53.34) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 52.07) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 49.53) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 48.26) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 46.99) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 45.72) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 43.18) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 41.91) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 40.64) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 39.37) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 36.83) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 35.56) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 34.29) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 33.02) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 30.48) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 29.21) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 27.94) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 26.67) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 24.13) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 22.86) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 21.59) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 20.32) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 17.78) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 16.51) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 15.24) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 13.97) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 11.43) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 10.16) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 8.89) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 7.62) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 5.08) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 3.81) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 1.27) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 2.54) (size 0.8 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
)
