(module SOLDER_JUMPER_2 (layer F.Cu) (tedit 54860803)
  (tags "solder jumper bridge configuration")
  (attr virtual)
  (fp_text reference JP*** (at 0 -1.7) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value SOLDER_JUMPER_2 (at 0 1.65) (layer F.SilkS) hide
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start 0.95 -0.6) (end 0.95 0.55) (layer F.SilkS) (width 0.2))
  (fp_line (start -0.7 -0.85) (end 0.7 -0.85) (layer F.SilkS) (width 0.2))
  (fp_line (start -0.95 0.6) (end -0.95 -0.6) (layer F.SilkS) (width 0.2))
  (fp_line (start -0.65 0.85) (end 0.65 0.85) (layer F.SilkS) (width 0.2))
  (fp_arc (start -0.7 0.6) (end -0.7 0.85) (angle 90) (layer F.SilkS) (width 0.2))
  (fp_arc (start -0.7 -0.6) (end -0.95 -0.6) (angle 90) (layer F.SilkS) (width 0.2))
  (fp_arc (start 0.7 -0.6) (end 0.7 -0.85) (angle 90) (layer F.SilkS) (width 0.2))
  (fp_arc (start 0.7 0.6) (end 0.95 0.6) (angle 90) (layer F.SilkS) (width 0.2))
  (pad 2 smd rect (at 0.4 0) (size 0.6 1.2) (layers F.Cu F.Mask)
    (clearance 0.1))
  (pad 1 smd rect (at -0.4 0) (size 0.6 1.2) (layers F.Cu F.Mask)
    (clearance 0.1))
)
