(module BUZZER_SMT (layer F.Cu) (tedit 57151A54)
  (fp_text reference REF** (at 0.1524 5.9436) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value >NAME (at -0.0508 -5.715) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user + (at -1.7018 -1.9558) (layer F.SilkS)
    (effects (font (size 2 2) (thickness 0.5)))
  )
  (fp_line (start -6 -6) (end -6 6) (layer Eco1.User) (width 0.15))
  (fp_line (start 6 -6) (end -6 -6) (layer Eco1.User) (width 0.15))
  (fp_line (start 5 5) (end 5 -5) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 6) (end 6 6) (layer Eco1.User) (width 0.15))
  (fp_text user + (at -5.461 -5.6134) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (fp_line (start 6 6) (end 6 -6) (layer Eco1.User) (width 0.15))
  (fp_line (start 5 -5) (end -5 -5) (layer F.SilkS) (width 0.15))
  (fp_line (start -5 -5) (end -5 5) (layer F.SilkS) (width 0.15))
  (fp_line (start -5 5) (end 5 5) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -3.5 -3.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 3.5 -3.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.5 3.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.5 3.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask))
)
