(export (version D)
  (design
    (source /home/dbroqua/Webstorm/dbroqua/DK60/DK60TP/Kicad/MouseButtons/MouseButtons.sch)
    (date "Fri 02 Jun 2017 07:32:09 PM CEST")
    (tool "Eeschema 4.0.5+dfsg1-4")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source MouseButtons.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref K1)
      (value K43)
      (footprint Footprint:Mx_Alps_100)
      (libsource (lib keyboard_parts) (part KEYSW))
      (sheetpath (names /) (tstamps /))
      (tstamp 593156D7))
    (comp (ref K2)
      (value K43)
      (footprint Footprint:Mx_Alps_125)
      (libsource (lib keyboard_parts) (part KEYSW))
      (sheetpath (names /) (tstamps /))
      (tstamp 59315811))
    (comp (ref K3)
      (value K44)
      (footprint Footprint:Mx_Alps_100)
      (libsource (lib keyboard_parts) (part KEYSW))
      (sheetpath (names /) (tstamps /))
      (tstamp 5931582D))
    (comp (ref K4)
      (value K45)
      (footprint Footprint:Mx_Alps_100)
      (libsource (lib keyboard_parts) (part KEYSW))
      (sheetpath (names /) (tstamps /))
      (tstamp 593158A2))
    (comp (ref K5)
      (value K45)
      (footprint Footprint:Mx_Alps_125)
      (libsource (lib keyboard_parts) (part KEYSW))
      (sheetpath (names /) (tstamps /))
      (tstamp 593158F2))
    (comp (ref D1)
      (value D)
      (footprint Footprint:D_SOD123)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 59315914))
    (comp (ref D2)
      (value D)
      (footprint Footprint:D_SOD123)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 593159AD))
    (comp (ref D3)
      (value D)
      (footprint Footprint:D_SOD123)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 593159F6))
    (comp (ref P1)
      (value CONN_01X04)
      (footprint Pin_Headers:Pin_Header_Angled_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 59315D1F)))
  (libparts
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp Diode_*)
        (fp D-*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib keyboard_parts) (part KEYSW)
      (fields
        (field (name Reference) K?)
        (field (name Value) KEYSW))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical keyboard_parts)
      (uri /home/dbroqua/Webstorm/dbroqua/DK60/Libraries/keyboard_parts.lib)))
  (nets
    (net (code 1) (name "Net-(D2-Pad2)")
      (node (ref K3) (pin 2))
      (node (ref D2) (pin 2)))
    (net (code 2) (name Col5)
      (node (ref K5) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref K4) (pin 1)))
    (net (code 3) (name Col4)
      (node (ref P1) (pin 2))
      (node (ref K3) (pin 1)))
    (net (code 4) (name Col3)
      (node (ref K1) (pin 1))
      (node (ref K2) (pin 1))
      (node (ref P1) (pin 3)))
    (net (code 5) (name Row4)
      (node (ref D1) (pin 1))
      (node (ref P1) (pin 4))
      (node (ref D3) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 6) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref K2) (pin 2))
      (node (ref K1) (pin 2)))
    (net (code 7) (name "Net-(D3-Pad2)")
      (node (ref K5) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref K4) (pin 2)))))