(module LED-3MM (layer F.Cu) (tedit 57232569)
  (descr "LED 3mm round vertical")
  (tags "LED  3mm round vertical")
  (fp_text reference LEDI3_2 (at 2.785 -4.045 270) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED (at 1.3 -2.9) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.77 -1) (end -0.23 -1) (layer Eco1.User) (width 0.15))
  (fp_line (start -0.23 -1) (end -0.23 1) (layer Eco1.User) (width 0.15))
  (fp_line (start 2.77 -1) (end 2.77 1) (layer Eco1.User) (width 0.15))
  (fp_line (start 2.77 1) (end -0.23 1) (layer Eco1.User) (width 0.15))
  (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  (model LEDs.3dshapes/LED-3MM.wrl
    (at (xyz 0.05 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
